[Lamp-MaxValue-Pct:INT0,100]
Output cap for Lamp.

Note this can be overridden by X\1 and X\2 commands.

Values range: 0-100

[Lux-OpenLoop-Opt:BOOL]
Specifies open loop or closed loop daylight dimming mode.

True: Open Loop
False:Closed Loop

[Lux-SetPoint-Lux:INT0,65535]
Specifies the setpoint for closed loop dimming, and the ??? value for open loop dimming.

This values is specified in Lux.  (Note values are approximate)

Value range: 0-65535

[Lux-Step-Pct:INT0,100]
Specifies the step used in closed loop dimming.

This value is specified in dimming percentage.  

Value range: 0-100

[Lux-Hysteresis-Lux:INT0,65535]
Specifies the size of the dead band in closed loop dimming.

This values is specified in Lux.  (Note values are approximate) 

Value range: 0-65535

[Lux-PollingRate-Secs:INT0,65535]
Specifies the period of lux controller updates, i.e. 1 update every x secs.

This value is specified in seconds.  

Value range: 0-65535

[PIR-AbsenceMode-Opt:BOOL]
Controls whether the PD operates in Absence Mode(Off Only) or Presence Mode (On and Off).

True: Off Only
False: On and Off

[PIR-Timeout-Mins:INT1,109]
Specifies the PD timout duration in minutes.

Value range: 1-109

[PIR-OnValue-Pct:INT0,100]
Controls the value the occupancy controller turns On to.

Value range: 0-100

[PIR-OffValue-Pct:INT0,100]
Controls the value the occupancy controller turns Off to.

Value range: 0-100

Not all occupancy controllers support support this attribute.

[Switch-Dimming-Opt:BOOL]
Controls the mode of operation of a switch.

True: Dimming
False:Switching

[Scene-Button4-Pct:INT0,100]
SCPTsecondVal[0] for OneTenSix (80002D2200040430)
SCPTsceneNmbr[0] for MetroBusWire (80002D2200040448)
SCPTprimeVal[0] for Scene Controller (3251)

Value range: 0-100
[Scene-Button3-Pct:INT0,100]
SCPTsecondVal[1] for OneTenSix (80002D2200040430)
SCPTsceneNmbr[1] for MetroBusWire (80002D2200040448)
SCPTprimeVal[1] for Scene Controller (3251)

Value range: 0-100
[Scene-Button2-Pct:INT0,100]
SCPTsecondVal[2] for OneTenSix (80002D2200040430)
SCPTsceneNmbr[2] for MetroBusWire (80002D2200040448)
SCPTprimeVal[2] for Scene Controller (3251)

Value range: 0-100
[Scene-Button1-Pct:INT0,100]
SCPTsecondVal[3] for OneTenSix (80002D2200040430)
SCPTsceneNmbr[3] for MetroBusWire (80002D2200040448)
SCPTprimeVal[3] for Scene Controller (3251)

Value range: 0-100
[Scene-Button0-Pct:INT0,100]
SCPTsecondVal[4] for OneTenSix (80002D2200040430)
SCPTsceneNmbr[4] for MetroBusWire (80002D2200040448)
SCPTprimeVal[4] for Scene Controller (3251)

Value range: 0-100